|  |  |
| --- | --- |
| **MFLNRO FSR Standard Sign Design** | **Catalogue Item #:** |
| **Radio Channel Tab Type 2** | **Fi-008-13c** |
| |  |  | | --- | --- | | **A** **🢡** | **Type 2 – Stand Alone** |   Substrate: Aluminum (0.081) 5052-H38  Conforming to ASTM B209M  No. Sides: Single Sided  Size: 120cm x 30 cm  Font: ClearviewHwy (4-B)  Reflectivity: ASTM Type 1  Overlaminate: Optional  3M 1160 UV/Anti-Graffiti guard  or equivalent  Border: inset 1.0cm / 1.5cm  Corner Radius: 38mm  Hole Diameter: 12mm dia  Hole Mount: Center Mount | **Special instructions:**   * Provide the following when ordering:   + **Type 2** (Catalogue No. Fi-008-13b):  1. Specify RR Road Channel number [**no** frequency (MHz) or tone]   **RR -**  (from 1 – 35)   * Anti-graffiti Select: 3M 1160 UV /Anti-Graffiti guard or equivalent   or Not Required   * Proofs to be provided by supplier for MFR approval * Provide one of the following electronic files to the sign fabricator:  |  |  | | --- | --- | |  |  | |