|  |  |
| --- | --- |
| **MFLNRO FSR Standard Sign Design** | **Catalogue Item #:**  |
| **Radio Channel Tab Type 2** | **Fi-008-13c** |
|

|  |  |
| --- | --- |
| **A** **🢡** | **Type 2 – Stand Alone** |

Substrate: Aluminum (0.081) 5052-H38 Conforming to ASTM B209MNo. Sides: Single SidedSize: 120cm x 30 cmFont: ClearviewHwy (4-B)Reflectivity: ASTM Type 1Overlaminate: Optional 3M 1160 UV/Anti-Graffiti guard or equivalentBorder: inset 1.0cm / 1.5cmCorner Radius: 38mmHole Diameter: 12mm diaHole Mount: Center Mount | **Special instructions:*** Provide the following when ordering:
	+ **Type 2** (Catalogue No. Fi-008-13b):
1. Specify RR Road Channel number [**no** frequency (MHz) or tone]

**RR -**  (from 1 – 35)* Anti-graffiti Select: 3M 1160 UV /Anti-Graffiti guard or equivalent

orNot Required* Proofs to be provided by supplier for MFR approval
* Provide one of the following electronic files to the sign fabricator:

|  |  |
| --- | --- |
|  |  |

 |