|  |  |
| --- | --- |
| **FLNRORD FSR Standard Sign Design** | **Catalogue Item #:**  |
| **FSR Use Warning Sign** | **Fw-055-1 & 2** |
|

|  |  |
| --- | --- |
| **Type 1: Fw-055-1 🢡****Type 2: Fw-055-2🢡** |  |

* Substrate: Aluminum nominal thickness 2mm (0.081”, sign grade aluminum 5052-H38 conforming to ASTM B209M
* No. Sides: Single Sided
* Reflectivity: ASTM Type 1
* Overlaminate: required; 3M 1160 UV/Anti-Graffiti guard or equivalent

Sizes: * Small: 1220 X 610mm for FSRs speed < 30 km/hr
* Medium: 1830 X 915mm for FSRs speed < 60 km/hr
* Large: 2440 X 1220mm

Fonts: * Small: (from top down) ClearviewHwy 5B 91.5mm, ClearviewHwy 2B 52.5mm and ClearviewHwy 3B 65.5mm
* Medium: (from top down): ClearviewHwy 5B 137mm, ClearviewHwy 2B 88mm and ClearviewHwy 3B 99mm
* Large: (from top down): ClearviewHwy 5B 183mm, ClearviewHwy 2B 105mm and ClearviewHwy 3B 131mm

Border: * Small: inset 6.35mm / width 9.5mm
* Medium: inset 6.35mm / width 14.3mm
* Large: inset 6.35mm / width 19.1mm
* Corner Radius: Small: 38.1mm / Medium: 63.5mm / Large: 88.9mm

Mounting Holes: field drilled; side mount | **Special instructions:**[ ]  Sign Type 1 – for FSRs that are not maintained for vehicular use[ ]  Sign Type 2 – for FSRs that are being maintained for vehicular useSpecify the following when ordering:* Sign type & Size:

[ ] Fw-055-1u - 1220 X 610mm, or[ ] Fw-055-1 - 1830 X 915mm, or[ ] Fw-055-1x - 2440 X 1220mmor [ ] Fw-055-2u - 1220 X 610mm, or[ ] Fw-055-2 - 1830 X 915mm, or[ ] Fw-055-2x - 2440 X 1220mm* Anti-graffiti: 3M 1160 UV /Anti-Graffiti guard or equivalent
* Proofs to be provided by supplier for FLNRORD approval
* Provide the corresponding electronic file to the sign fabricator:

 |