|  |  |  |
| --- | --- | --- |
| **FLNRORD FSR Standard Sign Design** | **Catalogue Item #:** | |
| **FSR Use Warning Sign** | **Fw-055-1 & 2** | |
| |  |  | | --- | --- | | **Type 1:  Fw-055-1 🢡**  **Type 2:  Fw-055-2🢡** |  |  * Substrate: Aluminum nominal thickness 2mm (0.081”, sign grade aluminum 5052-H38 conforming to ASTM B209M * No. Sides: Single Sided * Reflectivity: ASTM Type 1 * Overlaminate: required; 3M 1160 UV/Anti-Graffiti guard or equivalent   Sizes:   * Small: 1220 X 610mm for FSRs speed < 30 km/hr * Medium: 1830 X 915mm for FSRs speed < 60 km/hr * Large: 2440 X 1220mm   Fonts:   * Small: (from top down) ClearviewHwy 5B 91.5mm, ClearviewHwy 2B 52.5mm and ClearviewHwy 3B 65.5mm * Medium: (from top down): ClearviewHwy 5B 137mm, ClearviewHwy 2B 88mm and ClearviewHwy 3B 99mm * Large: (from top down): ClearviewHwy 5B 183mm, ClearviewHwy 2B 105mm and ClearviewHwy 3B 131mm   Border:   * Small: inset 6.35mm / width 9.5mm * Medium: inset 6.35mm / width 14.3mm * Large: inset 6.35mm / width 19.1mm * Corner Radius: Small: 38.1mm / Medium: 63.5mm / Large: 88.9mm   Mounting Holes: field drilled; side mount | | **Special instructions:**  Sign Type 1 – for FSRs that are not maintained for vehicular use  Sign Type 2 – for FSRs that are being maintained for vehicular use  Specify the following when ordering:   * Sign type & Size:   Fw-055-1u - 1220 X 610mm, or  Fw-055-1 - 1830 X 915mm, or  Fw-055-1x - 2440 X 1220mm  or  Fw-055-2u - 1220 X 610mm, or  Fw-055-2 - 1830 X 915mm, or  Fw-055-2x - 2440 X 1220mm   * Anti-graffiti: 3M 1160 UV /Anti-Graffiti guard or equivalent * Proofs to be provided by supplier for FLNRORD approval * Provide the corresponding electronic file to the sign fabricator: |